# Exchange Server 2003 Configuration

To configure VPIM on the Microsoft Exchange Server 2003:

To configure Email Connectors for VPIM:

1. Click Start > Programs > Microsoft Exchange > System Manager.

2. Expand Connectors, and then click Action > New > SMTP Connector.

3. On the General tab:

1. - In the Name field, type a descriptive name for the email connector (for example, "Connect to NPM").

   - Select Forward all mail through this connector to the following smart hosts:

   - Type the IP address of the host, in the following format (include the square brackets): [xxx.xxx.xxx.xxx]

   - Click Add to add Local Bridgehead. Select the local server and then click OK.

   - Click OK again.

4. On the Address Space tab, click Add, and then select SMTP and click OK.

5. In the Internet Address Space Properties window, you must now create one email domain address for the NuPoint UM (for the host):

   - In the E-mail domain field, type the fully qualified domain name (in the format servername.domain.com), and then click OK.

6. In the Internet Address Space Properties window, you must now create:

7. one email domain address for the NuPoint UM Standard (for the host):

OR

4. three email domain addresses for the NuPoint UM 640 (one each for the cluster, server 1, and server 2) or one email domain address for the NuPoint UM Standard (for the host):

1. - In the E-mail domain field, type the fully qualified domain name (in the format servername.domain.com), and then click OK.

   - For the NuPoint UM 640, repeat this step for the remaining two email domain addresses.