# DRAFT B (Internal) Changes for Release 4.2

The following topics have been changed/added for Release 4.2 (Draft B):

Features
Help Topic | New Topics | Updated Topics | Notes
About NuPoint UM Documentation |  | About the NuPoint UM Documentation | Listed the topics covered in each NuPoint UM document/Help file
What's New for Release 4.2 |  | Release 4.2 | Added description of new Client Throttling policies and configuration procedure that allows users increased access to the MAPI Gateway.
About NP Fax Applications |  | About NP Fax Applications | Added a note on the limitations of Windows 7 Re: opening .TIFF files using Photo Viewer or Microsoft Paint
Description (for Unified Messaging) |  | Description_UM | Augmented Unified Messaging Limits description: Completely disables FCOS bit 289 Overrides FCOS bit 304 and prevents notifications for email addresses for which a notification method other than Text Notification was selected Limits FCOS bit 304 to Text Notification only for email addresses for which Text Notification was selected
Configuring NP WakeUp |  | Configuring NP WakeUp_txt | Added this step to configuring enhanced NP Wakeup Enter the number of seconds to pull back the call; default is 60.
The Text Console |  | The Web Console | Added this note: Two user accounts are supported: "Admin" and "root". Only one user can be logged in to the system, from one network computer only, at any given time.
Adjust Audio Stream Volume | Adjust Audio Stream Volume |  | Added procedures for enabling and disabling automatic gain control functionality
Configure Outloook Security Settings |  |  | Removed references to Outlook 2010
Create a Superuser Account for MS Exchange 2010 |  | Create a Superuser Account for Microsoft Exchange 2010 | Created new topic and added a procedure for configuring the Client Throttling Policy
Define an Active Directory User Data Source |  | Define an Active Directory User Data Source | Changed extAttribute to extensionAttribute in steps 10 and 11 Removed this text: default value is person/contact
Configure IP Connectivity |  | Configure IP Connectivity | Note: If you are using a serial-to-IP converter, you must configure PMS iPocket solutions with NuPoint UM in IP PMS Server Mode.
Install and Configure the Precidia iPocket232 |  | Install and Configure the Precidia iPocket232 | Added/altered these steps: Select E) Remote IP and enter the IP address of the NuPoint server. If you are using the NuPoint 640 model, enter the cluster IP address. Select F) Remote Port and specify the PMS TCP Port to connect to on the NuPoint UM IP Address.
Configuring UM-SMTP, UM-WebView, and Standard UM |  | Configuring UM-SMTP and Standard UM | Added this Note: To support the forwarding of emails to users who are not Advanced UM users, through the Outlook Client Plug-in you must configure the Smart Host. Emails are sent using SMTP forwarding through the NuPoint UM system, not the Outlook client.