# Inter-Tel Axxess SIP Server Configuration

An Inter-Tel Axxess system has one Call Processing (CP) node but can have multiple Internet Protocol Resource Cards (IPRCs). Up to 20 IPRCs can be configured on AWV, however, at least one IPRC must be programmed to communicate with the AWV server.

Use the following settings only when configuring AWV with an Inter-Tel Axxess system. Configure the Inter-Tel Axxess system first, and then configure the SIP server settings using the information from the Axxess system configuration.

#### To configure the SIP component for the Inter-Tel Axxess:

1. From the MiCollab Audio, Web and Video Conferencing main page, click System Options on the navigation pane.

2. In System Options – Platform, select Inter-Tel Axxess for the system connected to MiCollab Audio, Web and Video Conferencing.

3. Click Save, and then click Ok at the prompt to restart the server.

4. Click Configure SIP Server on the navigation pane. The Inter-Tel Axxess SIP Server Configuration page appears.

5. Enter the following information:

- Node Number: Type the node number of the Inter-Tel Axxess that is connected to MiCollab Audio, Web and Video Conferencing. If the Inter-Tel Axxess is configured as a single node, type 1, which is the default.

- OAI IP Address: Type the IP address of the Inter-Tel Axxess system.

- OAI Port: Type the port number used on the Inter-Tel Axxess for OAI. The default value is 4000.

- OAI Password: Type the password used to connect to OAI.

6. Type the following information for the IPRC you want to connect to MiCollab Audio, Web and Video Conferencing:

- IP Address: Type the IP address of the Inter-Tel Axxess IPRC.

- Extension First: Type the extension number of the first IP device used by the MiCollab Audio, Web and Video Conferencing server to register itself with the Inter-Tel Axxess.

- Extension Last: Type the extension number of the last IP device used by the MiCollab Audio, Web and Video Conferencing server to register itself with the Inter-Tel Axxess.

7. Do one of the following:

- If you are configuring another IPRC, click New IPRC, and then repeat step 6 to add the IPRC.

- If you are finished configuring the IPRC, click Save, and then click Ok at the prompt.

8. Verify the results of the SIP registration process, see Proxy Extension Status.