# Configuring the NuPoint UM Server for an IP Serial port

After the Precidia iPocket232 has been installed and configured, the NuPoint UM server must be configured to receive information from the PMS through the Precidia iPocket232.

## To Configure the Server for an IP Serial Port:

1. From the Main Menu, From the Main Menu, select (S) System Maintenance, (R) Reconfiguration, (R) Reconfigure System, and then (G) Offline Menu.

2. From the Offline Configuration Menu, select (B) Duplicate the Active Configuration.

3. Select (M) RS232 Only Applications.

4. Select (I) IP Serial Port Selected and enter the IP serial port index number.

5. At the IP serial Port IP Address prompt, enter the IP address of the Precidia iPocket232.

6. At the IP serial port's server port number prompt, enter the virtual port number you configured as the local and remote port number when configuring the Precidia iPocket232. You are returned to the RS232 Only Applications Menu.

7. Select your integration type (Hyatt, EECO or HIS). This selection automatically sets the appropriate serial port settings.

8. Exit to the Offline Configuration menu and select (X) Exit - Save Changes.

9. Activate the inactive configuration.

The NuPoint Unified Messaging server has been configured to communicate with the Precidia iPocket232. The Precidia iPocket232 can now be connected to the server. Proceed to configuration for EECO and HIS or Encore.