# LCOS Parameters and Default Values (Text Console)

LCOS 1 is pre-configured; it contains the default values for all parameters. All mailboxes are assigned LCOS 1 by default, unless otherwise configured by the system administrator.

The tables below provide a quick reference to all the limits parameters, with default values.

Limits Parameters Menu | Default Value
(G) Greeting length | 2.0 (minutes)
(N) User name length | 2 (seconds)
(M) Message count | 200*
(B) Messages per billing | 0 (no limit)
(L) User message length | 5.0 (minutes)
(C) Caller message length | 5.0 (minutes)
(E) End of message warning time | 0 (seconds)
(T) Maximum login time | 0 (no limit)
(O) Maximum NP View Inactivity Timeout | 59 (minutes)
(W) Network queue message count | 99
(S) Maximum attachments per message | 199
(I) Maximum attachments per network message | 199
(D) Message delivery login delay | 5 (seconds)
(P) Mailbox passcode expiry | 0=disabled (days)

More Limits Parameters Menu | Default Value
(A) NP WakeUp - phone length | 11 (digits)
(B) Paging - phone length | 11 (digits)
(C) Message delivery - phone length | 11 (digits)
(D) Future delivery - message count | 99
(E) Max days - future delivery | 60 (days)
(F) Max family member or guest | 0 (not used)
(G) Message waiting indicator - message length | 0 (no minimum)
(H) Minimum message length | 0 (no minimum)
(I) Maximum pages per billing | 0 (no limit)
(J) Maximum wakeups per billing | 0 (no limit)
(K) Maximum outstanding wakeup calls | 0 (not used)
(L) Callback number length | 11 (digits)

Even More Limits Parameters Menu | Default Value
(A) Max days - NP WakeUp | 0 (no limit)
(B) Max days - reminder call | 0 (not used)
(C) Max reminder calls per billing | 0 (not used)
(D) Max destinations per reminder call | 0 (not used)
(E) Max members per distribution list | 200
(F) Max recipients count | 190 (per message)
(G) Max number of distribution lists | 99 (lists)
(H) Min number of recipients for receipt summary | 0 (no recipients)
(I) Minimum billed number length | 0 (digits)
(J) Max hours to wait for reply from NIB | 0 (not used)

Call Placement Menu | Default Value
(A) Ring No Answer (RNA) retry limit | 5 (retries)
(B) RNA retry interval | 5 (minutes)
(C) Busy retry limit | 5 (retries)
(D) Busy retry interval | 5 (minutes)
(E) Message phone length | 11 (digits)
(F) Recipient count | 190
(G) Maximum message length | 5 (minutes)

Fax Limits Parameters Menu | Default Value
(A) Maximum Number of digits for telephone number | 11 (digits)
(B) Fax Message count | 199 (quantity)
(C) Pre-greet silence interval to improve walkaway CNG detection | 0 (seconds)
(D) Fax delivery retry frequency | 5
(E) Fax delivery retry interval | 5 (minutes)

Message Retention Limit Menu | Default Value
(M) Message retention | 0 (no limit)
(P) Played message retention | 672 (hours)
(U) Unplayed message retention | 336 (hours)
(R) Urgent message retention | 336 (hours)
(S) Cut-through paging receipt retention | 672 (hours)
(T) Receipt retention | 672 (hours)
(A) Played Fax Message Retention | 672 (hours)
(B) Unplayed Fax Message Retention | 336 (hours)
(C) Urgent Fax Message Retention | 336 (hours)
(D) Fax Receipt Retention | 672 (hours)
(E) Absolute message retention | 0 (no limit)

Prompt Language Selection Menu | Default Value
(D) Use default |
Other Prompt set options are listed according to the optional features installed. |

*For systems that upgrade to release 4.1 or later from a pre-4.1 release, this LCOS parameter carries forward a default of 73 messages.