# Programming an Analog Services Unit II (ASU II)

## Before You Begin

Ensure that the Analog Services Unit is connected as shown in the Technician's Handbook.

## Programming

To program an ASU II:

- Analog Services Units form

- Click Change and Select "ASU II" from the Programmed Type field.

- In the Programmed Card Slot 1 field, select the installed analog card type.

- In the Programmed Card Slot 2 field, select installed analog card type. Valid analog card types are "24 Port ONSP Card", "16 Port ONS Card", or "4 + 12 Port Combo Card".

NOTE: You must purchase an analog line license for each ONS port on an analog card. Check the Analog Line Licenses fields in the System Capacity form ( ) to determine the number of available licenses. Subtract the number of used licenses from the number of purchased licenses.

Related Topics

- Program a Universal ASU

- Program an ASU

- Program Embedded Analog

- Program Analog Telephones

- Program Analog Trunks