# RMESS

## Qualifiers:

VERIFY PBX <pbx number> LAN

VERIFY PBX <pbx number> PPP

## Purpose:

Verifies remote message link establishment.

## Details:

The VERIFY qualifier attempts to establish a remote message link to the specified PBX. After the connection is made, a test is performed to see if the PBX is programmed with the specified PBX number as its Local PBX Number. When the test is complete, the remote message link is disconnected and a response is made to the maintenance terminal.

The LAN or PPP qualifiers designate the transport type.

The Rmessage command relies on appropriate programming in the ICP/PBX Networking and XNET ICP/PBX Networking forms.

## Example:

### Entry: RMESS VERIFY PBX 1 PPP

System Response:

Connected to PBX 1

NOTE: If the system response returns a failed function, a reason is provided. Possible reasons include: HDLC congestion, trunk congestion, invalid pbx id, invalid remote pbx id, invalid DID number, and timeout.