# DBTAB

## Qualifiers:

<table id>

<table id> <record id>

## Purpose:

The DBTAB command provides database table information and the ability to display the contents of a specific table record.

## Details:

DBTAB <table id> - displays information about the requested database table. Table id 0 (zero) contains a list of all database table ids.

DBTAB <table id> <record id> - displays the binary contents of the specified table record.

## Examples:

Entry: DBTAB 0

System Response:

1 ($01) sws_receiver - record level support
2 ($02) sws_station - record level support
3 ($03) sws_ss4 - record level support
4 sws_data_station - record level support
5 ($06) sws_mfr_group - table level support
6 ($07) sws_ansDvc_group - record level support
7 ($08) sws_trunk - record level support
8 ($09) sws_trk_group - record level support
<numerous fields not shown>

Entry: DBTAB 1

System Response:

1 ($01) sws_receiver[0.. 127] Record size: 5
Address: 025007D8 Bit map pointer: $00AA3124 Table cardinality: 48

Entry: DBTAB 1 1

System Response:

sws_receiver [ 1 ] =
0E 0F 00 01 02 03
025007DE: 00 03 1C 01 00 00 ......