# STP Default Settings (700-user, 250-user Controllers)

When STP is enabled, MiVoice Business uses the following STP configuration values by default:

Parameter | Description | Default Value
Port enabled (each of L2 external ports 1-4) | True |
L2 STP Fast Convergence | False |
Path Cost (all ports) | 10 |
Port Priority (all ports) | 255 |

NOTE: The defaults are those specified in the standard. For more information, refer to the IEEE 802.1D specification.