# DSP Status Alarm

## System/Sub-System

MiVoice Business: Hardware

## Description

Indicates that a percentage of DSP resources are unavailable.

### Details

This alarm applies only to 3300 ICP controllers.

## Alarm Status

The minor threshold is 1. The critical threshold is 100.

#### Possible Cause | #### Corrective Action
--- | ---
The failure of one or more, but not all, DSPs, or a system configuration issue results in a Minor alarm. A Critical alarm indicates that all DSPs have failed. The DSP licenses are enabled but not enough DSP resources are available to support compression requirements. Faulty circuit on DSP module. | Use the SHOW STATUS DSP maintenance command to determine if any DSPs have failed. If indicated, replace defective DSP module. See the Engineering Guidelines to check if required hardware is installed for the configuration of the system and/or see “Increasing DSP Resources” in the “Installation Planner” chapter of the Technician’s Handbook for instructions. If indicated installed required DSP cards.