# Gateway Sets (EX Controller)

## Purpose:

The Gateway Sets form is a read-only form. This form displays the list of analog devices that are connected to the MiVoice Business network through the Open Network Service (ONS) ports on the EX controller. The SIP Device Capabilities form lists the device type of the newly added devices as Analog FXS.

If the destination number (DN) of an analog device is programmed in the MiVoice Business system, it is displayed in the Number field. If not, a blank field is displayed under the Number field.

NOTE: This form is applicable only to the EX Controller.

## Field Descriptions

Parameter | Description | Default Value
Gateway | Indicates the IP address of the EX Controller. | Not applicable
Endpoint ID | Indicates the physical location of the end point. | Not applicable
Number | Indicates the DN of the gateway set. | Blank

Related Topics

- Programming Analog Sets on an EX Controller

- Programming Analog Telephones

- Programming Analog trunks