# Gateway PRI Configuration

# (Mitel Integrated Configuration Wizard)

The Gateway PRI Configuration page enables you to change the PRI line type and PRI signaling method for a PLID.

NOTE: This configuration is applicable only for EX platforms.

To change the PRI line type:

1. Locate the PLID for which you want to change the PRI line type. For this PLID, select a value from the PRI Line Type drop-down list.

NOTE: PLIDs are auto-detected by the system and displayed on the Gateway PRI Configuration form. This field is non-configurable.

2. The system displays a notification message, before reboot. Click Continue.

3. After reboot is completed, the PRI Line Type you selected is applied to the PLID. Click Next to continue.

To change the PRI signaling method:

1. Locate the PLID for which you want to change the PRI signaling method. For this PLID, select a value from the PRI Signaling drop-down list.

2. The system displays a notification message, before reboot. Click Continue.

3. After reboot is completed, the PRI signaling method you selected is applied to the PLID. Click Next to continue.