# Programming System Printer Ports

To program system printer ports:

1. System Ports form

- Assign a logical name to the system port.

2. Application Logical Ports form

- Assign an LPR1 telnet port to each application. The application records or logs are captured on the LPR1 port, which can be viewed using a terminal emulator application, such as a PuTTY.

See also Printer Support for information on configuring MiVoice Business to use a network printer.