# SYSTEM TOTALS

## Qualifiers:

None

## Purpose:

Displays the total number of programmed trunks, lines, stations, and attendants (with a breakdown by device type).

## Details:

The information provided by this command is used by PTT for charging purposes and, as such, accurately reflects the number of programmed extensions and trunks currently being used by the system.

Any station or trunk that has been assigned an extension number or a trunk number in their respective programming forms will be considered programmed.

The circuits included in the totals will not necessarily be in a working state. The totals will include circuits in manbusy, under test, or in an indeterminate state.

Device types with zero programmed circuits (i.e. the database has none of these devices programmed) will not be included in the breakdown of the totals.

## Example:

### Entry: SYSTEM TOTALS

System Response:

TOTAL TRUNKS | 116 | TOTAL STATIONS | 623
TOTAL ATTENDANTS | 1 |  |
E&M Trunks | 1 | UNIVERSAL T1 Trunks | 115
On Premise Stations | 67 | Off Premise Stations | 3