# LOCATE TRUNK

## Qualifiers:

<trunk number>

## Purpose:

Locates the specified trunk.

## Details:

When the LOCATE TRUNK command is invoked on a trunk circuit belonging to a trunk group, the trunk group number to which the trunk belongs is displayed, and the set of groups that contains the group with the located trunk is displayed (as illustrated in the example).

When the located trunk does not belong to a trunk group, the following response message is displayed:

Trunk does not belong to any Trunk Group.

## Example:

### Entry: LOCATE TRUNK 1

System Response:

Card Type: Universal T1
Circuit Location: 6 1 1 1 1
Trunk Number 1 is assigned to: 6 1 1 1 1
Trunk does not belong to any Trunk Group