# Timed Recall (TI/D4)

The Timed Recall feature provides a timed recall for unanswered calls and calls transferred to a busy extension in the following instances:

- an incoming trunk or station call is transferred across the network to a station or trunk which does not answer

- an incoming trunk or station call is transferred across a digital network to a busy device.

The party who invoked the transfer receives the recall after a programmable period as defined in the No Answer Recall Timer or the Camp-on Recall Timer fields of the class of service assigned to the local outgoing digital trunk.

This feature is not subject to conditions, programming, or operation instructions.