# REMOVE COURTESY DOWN

## Qualifiers:

<unit> <shelf> <slot> <circuit>

EXTENSION <extension number>

## Purpose:

Cancels the Courtesy Down operation requested during a busying operation and subsequently found to be unnecessary.

## Details:

Courtesy Down requests are automatically removed upon logout from a maintenance session.

The EXTENSION qualifier allows courtesy down to be canceled by specifying the extension of a set. System Response is the same whether an extension or Location ID is used. If the extension is the prime member of a Multi-device User Group or PRG, the system response will include the following message: "This number refers to a <Multi-device User Group | Personal Ring Group>."

## Examples:

### Entry: REMOVE COURTESY DOWN 1 1 1 3

System Response:

Removed Courtesy Down request for circuit at location 1 1 1 3

### Entry: REMOVE COURTESY DOWN EX 6001

System Response:

Removed Courtesy Down request for circuit at location 1 2 2 6

### Entry: REMOVE COURTESY DOWN EX 26004

System Response:

The number refers to a Multi-device User Group.
Pilot Number: 26004
Members: 26004,26002,1020
Removed Courtesy Down request for circuit at location 2 6 0 0 4