# Printer Support

## Description

The system supports a telnet port (LPR1) that can be programmed to view:

- Maintenance Logs

- SMDR Logs

- ACD Logs

- Software Logs

- Hotel/Motel Logs

Support is also provided for SFTP (spooler) network printing of the following :

- Hotel/Motel reports

- Traffic reports

- SMDA

## Conditions and Feature Interactions

- Network printers must support the use of FTP for spooling print jobs.

## Programming

To enable output from LPR1 telnet port:

- Assign LPR1 to applicable logs in the Application Logical Ports form.

To enable printing to a network printer

1. Controller Registry form

- Program the network printer connection parameters.

2. System Ports form

- Assign a name to the network port.

3. Application Logical Ports form

- Assign to applicable logs.

## Device Support

Not applicable

## Operation

None