# Multiline Advisory Messages

## Purpose

The Multiline Advisory Messages form defines up to 20 status messages that may appear on display telephones.

Use this form when performing the following tasks:

- Messaging - Advisory

- Language Change

## Field Descriptions

Parameter | Description | Default Value
Language | Select one of the following languages; English, French, German, LA-Span, Dutch, Italian, Romanian, PT-Portuguese, EU-Span, and Russian. NOTE: Status messages are not supported in Swedish, Polish, Simplified Chinese, Local 1 and Local 2. | Blank
Languages Currently Loaded | System-generated, protected field. This entry is generated by the system during data entry and need not be completed. Only three versions (languages) of the form are kept in the system. |
Messages |
Message Number | A number in the range 1 to 20 used to identify the messages internally. Messages in each language should parallel one another (for example, Message Number 1 should mean the same in French, Italian, German, Spanish, Portuguese, or Dutch as the English message). |
Message | Enter a message. | Blank