# LOCATE PLID

## Qualifiers:

<unit> <shelf> <slot>

<unit> <shelf> <slot> <circuit>

<unit> <shelf> <slot> <circuit> <channel>

## Purpose:

Generates information about the circuit specified by the given Physical Location IDentifier (PLID).

## Details:

When the located trunk does not belong to a trunk group, the following response message is displayed:

Trunk does not belong to any trunk groups.

For Hot Desk user DNs, the MAC Address does not apply.

## Example:

### Entry: LOCATE PLID 1 3 1 1 1

System Response:

IP Device ID: 1
Circuit Location : 1 3 1 1 1
Extension : 4000
MAC Address: 08:00:0F:00:A2:FC
Active Zone: 3