# Station Attributes

## Purpose

Use the Station Attributes form to assign a Class of Service, Class of Restriction, Intercept Number, and Default Account Code number to each station in the system. This form uses Range programming.

NOTE: When an IP Phone is added to the system as a Userless Device
An IP device configured with service level "IP Device Only"; provides basic functionality (emergency/attendant calls and hot desk login) and does not require a license. using the Automatic DN Selection registration method, the system auto-configures various fields in this form. See Registering and Auto-provisioning Multiline IP Telephones without a DN for details. You can change these configuration values after the device is registered.

The Station Attributes form refers to the following forms:

- ONS/OPS Circuit Descriptors form

- Multiline IP Sets form

- Single Line IP Sets form

- IP Consoles form

- Class of Service Options form

- Network Zone Topology

The Class of Restriction numbers defined in this form are referenced by the Class of Restriction Groups form.

A station may have a different Class of Service and/or Class of Restriction for each mode of service: Day, Night 1, and Night 2.

## Field Descriptions

Parameter | Description | Default Value
Number | System-generated, protected field. Lists directory numbers. |
Intercept Number | Enter the Intercept Number from the Intercept Handling form. | Blank
Class of Service - Day | Enter a COS number for Day mode of service. | Blank
Class of Service - Night1 | Enter a COS number for Night1 mode of service. | Blank
Class of Service - Night2 | Enter a COS number for Night2 mode of service. | Blank
Call Coverage Service Number | Enter the Call Coverage Service Number from the Call Coverage Services form. | 1
Class of Restriction - Day | Enter a COR number for Day mode of service. | Blank
Class of Restriction - Night1 | Enter a COR number for Night1 mode of service. | Blank
Class of Restriction - Night2 | Enter a COR number for Night2 mode of service. | Blank
Default Account Code | Enter a code from the Default Account Codes form. | Blank
Zone Assignment Method | Select the Zone Assignment method: Default or Manual. When Default is selected, the Zone ID doesn't have to be entered because the zone of the MiVoice Business system to which the set is registered is used. If you selected Manual, you must enter the Zone ID in the Zone ID field. The Zone ID information can also be configured in the User and Services Configuration form. NOTE: Always use Manual if this form is shared with a 3300 ICP Release 7.0 system. | Default
Zone ID | Enter the Zone ID in the range 1 to 999 for the associated IP device DN. Compression is not applicable to non-IP devices. | 1 (default zone)
SIP Device Capabilities | The number of the SIP Device Capabilities form that corresponds to this station. Non-SIP devices ignore this value. | 1