# Using CoA Provisioning Files to Configure Mitel SIP-DECT Phones

## Overview

Configuration over Air (CoA) for Mitel SIP-DECT allows you to

- Configure phone settings (e.g. language, ring behavior, messaging, etc.)

- hide, gray out, lock or PIN protect menus

- configure softkeys

With SIP-DECT 6.1 this capability has been enhanced to also deploy customizable phone menus.

Up to two menus (variable lists) with each containing up to 10 entries can be configured in a configuration profile.

In the example below, a Call services menu has been added to enable or disable MiVoice Business call control features.

The menu is accessible when the phone is in idle state via a “more” softkey. Depending on the feature, the phone either prompts for user input or invokes the feature in question.

### Deployment Example for MiVoice Business

Idle | Menu (EN) | User Input

## Requirements

- SIP-DECT Release 6.1 or higher

- 602 DECT Phones with Software 6.1 or higher

- CoA provisioning file from repository (pbx_menu_coa.zip)—e.g., mivb_menu_en.coa

## Configuration

CoA provisioning files in the repository contain a list features and feature access codes (FACs).

The codes in the provisioning files must match the feature access codes configured in MiVoice Business.

Modify the CoA file or the MiVoice Business feature access codes to match each other if required.

NOTE: The files are provided with the default MiVoice Business FACs already in them.

Edit the configuration files with a text editor such as Notepad. Editing requirements and notes are included in the files themselves.

For more information on CoA, see the Mitel SIP-DECT OM System Manual available on Mitel Document Center website.

### Templates

A repository with sample provisioning files is included in the pbx_menu_coa.zip file.

Download the repository file using the following link:

http://gsd.aastra.com/SIP-DECT/COA/pbx_menu_coa.zip?encoded=0518cc01d55094151be6c

The following table is an overview of feature codes by region. The codes are based on the MiVoice Business default FAC v.13.2.

Table 1: mivb_menu_<region>_<language>.coa - defaults

Feature Code | Legacy | US/ CAN | DE/ BE/ NL | UK/ FR/ AUS/ Other | NZ | Action on click
Call Forward | **8 | *355 | *21 | *64 | *31 | Input + dial
Call Forward Cancel | ##8 | #350 | #29 | *70 | **30 | Dial
Do Not Disturb | *5 | *370 | *25 | *06 | *11 | Dial
Do Not Dist. Cancel | #5 | *371 | #25 | #20 | **11 | Dial
Call Pickup | *6 | #44 | **3 | *53 | *8 | Dial
Call Park Retrieve | *8# | *0 | ###8 | *52 | **7 | Input + dial
Direct/Group Page | *37 | #7 | *41 | #** | ##* | Input + dial
Loudspeaker Page | **9 | *7 | **9 | *01 | *06 | Dial

The phone menu is available in different languages.

Deploy the file matching to your region and language.

Table 2: mivb_menu_<region>_<language>.coa

Region | Matching countries using default FAC
us_can | US = USA CAN = Canada
de_be_nl | DE = Germany BE = Belgium NL = Netherlands
uk_fr_aus_other | UK = United Kingdom FR = France AUS = Australia other = other regions
nz | NZ = New Zealand
legacy | legacy = codes for backward compatibility reasons to other Mitel DECT solutions

Language Code | Language
EN | English
FR | French / Francais
DE | German / Deutsch
NL | Dutch . Nederland

### Mitel SIP-DECT Configuration

1. Connect to the OMM using OMP and create a new CoA Profile.

OMP > Configuration > System features > CoA Profiles

- If this CoA profile is to apply to all 602 DECT Phones in this system, enable the “Default” checkbox.

- If this profile should only apply to specific users, define a Profile Name. Use Import file to upload the required coa file.

- If the profile was not set as “Default” users must be assigned to use this profile. Go to OMP > Configuration > DECT Phones > Users.

2. Select the user(s) you want to apply this profile to and click on configure.

3. Switch to the configuration data tab and select the profile you want to apply.

4. To provide the menu in different languages create multiple CoA profiles and manually assign the CoA profile with the correct language to the user.

### MiVoice Business Configuration

Confirm that all required feature access codes are configured in the Feature Access Codes form.

Related Topics

- Programming Mitel SIP-DECT Phones

- Recommended SIP Peer and Device Capatibility Settings