# VM Network Servers

## Purpose

The VM Network Servers form is used to program and manage VM Network Servers. Up to 200 voice mail servers can be programmed.

Use this form when performing the following tasks:

- Programming Networked Voice Mail

- VM Network Users

For more information:

- About Networked Voice Mail

## Field Descriptions

Parameter | Description | Default Value
Network Element Name | The host name of the voice mail server, as defined in the Network Elements form. This field can have up to 9 characters. NOTE: The name that you enter in this field must match exactly with the name that is assigned to the element in the Network Elements form; otherwise, you will be unable to add or edit extension mailboxes. | Blank
Network Element Type | The type of voice mail server. | 3300 ICP
Local | Select "Yes" if this voice mail server is on this ICP. Only one server can be set to "Yes". | Blank
Cluster | Select "Yes" if this ICP belongs to a cluster. | Blank
PNI | Enter the Primary Node ID of the cluster to which this ICP belongs. This field can have up to 7 digits. | Blank
Server Address | The IP address or FQDN of this ICP, as defined in the ICP/PBX Networking form. | Blank
DNS Name | The DNS name of this ICP. This field can have up to 255 characters. | Blank
Time Zone | The time zone of this ICP (compared to GMT). TIP: Set this time to match your own time zone to ensure that the timestamps on your voice mails, and the sent times on any voice mails forwarded to email, are reported correctly. | GMT - 4:00
Comment | This field can have up to 255 characters. (Optional) | Blank