# Account Codes - System

## Description

System Account Codes are automatically outpulsed by the system when outgoing calls are made on specialized carrier trunk circuits. When a user makes a call on one of these circuits, the System Account Code is outpulsed by the system and used by the carrier to validate and record details of the call.

## Conditions and Feature Interactions

- You can program the System Account Code to be outpulsed either at the beginning or the end of the digit stream.

- The System Account Code must be referenced on the modified digits table for the appropriate ARS route.

- A maximum of 24 system account codes may be programmed.

## Programming

1. Program the Account Code Numbers in the System Account Codes form.

2. Enter the associated Account Code Index numbers in the ARS Digit Modification Plans form.

## Device Support

Not applicable

## Operation

None

Related Topics

- Account Codes - Default

- Account Codes - Verified and Non-verified