# Configuring Controller Modules and Framers
(Mitel Integrated Configuration Wizard)

To configure controller modules and framers:

1. Select Configure Controller Modules and Framers.
   If the check box is cleared, all field entries are ignored.

2. Click and select each Programmed Module Type.

3. Click and select the interface type on each port for the T1/E1 Combo Card or Dual T1/E1 Framer.
   The T1/E1 Combo Card uses port 1 only. By default, the Quad BRI Framer provides 4 ports with a BRI interface.

NOTE: The controller modules and framer configuration is not applicable for EX platform.

4. Click Next to continue.