# Attendant Trunk Group Status Display (Traffic Monitoring)

## Description

Attendant Trunk Group Busy Status Display lets you display the busy status of the system trunk groups from the attendant console. The busy status display is a 'snapshot' of the current usage of outgoing trunk groups. Trunk groups may be specified by group number or leading digits.

## Conditions and Feature Interactions

- Not available on the MiVoice Business Console.

## Programming

Program a TRUNK GROUP STATUS firmkey (see Attendant Console Firmkeys).

## Device Support

5540 IP Console

## Operation

#### 5540 IP Console

To view the status of all trunk groups:

1. Press Trunk Stat.

2. Press Trunk Groups.

3. Press Enter.

4. Do one or more of the following:

5. To view the trunk groups, press Next and Previous.

6. To update the displayed information, press Update Status.

7. To return to attendant mode, press Exit.

To view the status of a specific trunk group:

1. Press Trunk Stat.

2. Press Trunk Groups.

3. Enter the trunk group number.

4. Press Enter.

5. Press Exit.

To view a trunk group by specifying the trunk access code and ARS Digits Dialed:

1. Press Trunk Stat.

2. Press Digits Dialed.

3. Enter the trunk access code.

4. Enter the ARS Digits Dialed.

5. Press Enter.

6. Press Exit.

To print the displayed information:

1. Press Print Screen.

2. Press Exit.

To print all trunk group information while you are viewing the status of all trunk groups:

1. Press Print All.

2. Press Exit.