# Bootrom Alarm

## System/Sub-System

MiVoice Business: Hardware

## Description

There is bootrom version mismatch.

## Alarm Status

The minor threshold is 100.

#### Possible Cause | #### Corrective Action
--- | ---
Hard disk or processor card replacement. | Upgrade the firmware in the card from the version on the system hard drive. Run the UPGRADEBOOTROM ALL maintenance command to upgrade the firmware. After the command is executed, the system prompts you to reboot the controller. Run the RESET SYSTEM maintenance command for the new firmware to take effect.