# Line Type Values

Value | Description
Account Code Non Verified | The key is programmed as an Account Code key for non-verified account codes.
Account Code Verified | The key is programmed as an Account Code key for verified account codes.
ACD | This is key programmed as an ACD agent log in/log out key
Analog Line | This key is programmed to access an analog line on a telephone with a Line Interface Module attached.
Application | The key is programmed as an application (for example, as a video key for 5700 Voice First Application or VCON Video Conferencing).
Auto Answer | The key is programmed as an Auto Answer key.
Call Fwd Always | The key is programmed as a Call Forward - Always feature access key.
Call Fwd Busy | The key is programmed as a Call Forward - Busy feature access key.
Call Fwd Busy External | The key is programmed as a Call Forward - Busy (External Source) key.
Call Fwd Busy Internal | The key is programmed as a Call Forward Busy - (Internal Source) feature access key.
Call Fwd No Answer | The key is programmed as a Call Forward - No Answer feature access key.
Call Fwd No Ans. External | The key is programmed as a Call Forward - No Answer (External Source) key.
Call Fwd No Ans. Internal | The key is programmed as a Call Forward - No Answer (Internal Source) feature access key.
Call History | The key is programmed to turn-on or turn-off Call History recording on that set.
Call Park | This key is programmed as a Call Park feature access key.
Call Park – Retrieve | This key is programmed as a Call Park - Retrieve feature access key.
Call Pickup | The key is programmed as a Dialed Call Pickup key.
Callback | The key is programmed as a Callback key.
Campon | The key is programmed as a Camp-on key.
Cancel | This key is a Cancel key. (Used to end a call in progress and to discard inputs during a set programming session.
CDE Speedcall | The key is a Speed Call key programmed during system programming.
Direct Page | The key is programmed as a Direct Page key.
Do Not Disturb | The key is programmed as a Do Not Disturb key.
Double Flash | The key is programmed to send a double Trunk Flash.
DSS/Busy Lamp | The key is a Direct Station Select (DSS) key of the associated directory number while the corresponding appearance displays the status of the monitored device.
Emergency Call | The key is programmed as an Emergency Call Notification feature key.
Generic Group Alert | The key is an ACD Generic Threshold Alert indicator.
Group Listen | This key is programmed a Group Listen feature key
Group Park | This key is programmed as a Group Park feature access key.
Group Presence | This key is programmed as a Group Presence feature access key.
Handoff | The key is programmed as a Handoff key.
Headset | The key is programmed as a Headset key.
Hold | This key is programmed as a Hold key
Hot Desking | This key is programmed as a hot desking key. (Used to initiate a hot desk log in.)
Key System | The corresponding directory number is part of a key system group.
Make Busy | The key is programmed as a Make Busy key.
Meet-Me Answer | The key is programmed as a Meet-Me Answer key.
Message | This is a Message key. (Used on certain phones to request a Callback or respond to a message waiting indication)
Message Waiting Indication | The key is programmed as a message waiting indicator for a voice mailbox.
Microphone | This key is a Microphone key.
Mobile Line | This key is programmed as a Mobile Line key
Multicall | The corresponding directory number is part of a multicall group.
Music | The key is programmed as a Music key.
Night Answer | The key is programmed as a Trunk Answer From Any Station (TAFAS) key.
Night Service Indication | The key is programmed as a Night Service key.
Not Assigned | The key is not programmed in the System Administration Tool or by the user.
Override | The key is programmed as an Override key.
Paging | The key is programmed as a Paging key.
Personal Presence | This key is programmed to toggle the Group Presence state of a Personal Ring Group member.
Phone App | This key is programmed to launch an application (People, Call History, Visual Voice Mail, etc.) on 5320/5320e, 5330/5330e, 5340/5340e and 5360 IP Phones. NOTE:
Phone Lock | This key is programmed as a Phone Lock key.
Phonebook | This key is a Phonebook key.
Privacy Release | The key is programmed as a Privacy Release key.
Record a Call | The key is programmed as a Record-A-Call feature key.
Redial | This key is a Redial key.
Release | The key is programmed as a Release key.
Secretarial | The key allows secretarial transfer of calls on soft hold to the associated directory number as well as all DSS/busy lamp key functions.
Single Flash | The key is programmed to send a single Trunk Flash.
Single Line | The corresponding directory number is a single line.
Speaker | This key is a Speaker key.
Specific Group Alert | The key is an ACD Specific Threshold Alert indicator.
Superkey | This key is a Superkey.
Swap | The key is programmed as a Call Swap feature access key.
Tag Call | The key is programmed to invoke an SMDR record of the call.
Trans/Conf | The key is a Transfer/Conference key.
URL Line | The key is programmed to launch a web page or other resource from the specified URL.
User Speedcall | The key is a Speed Call key programmed by the user
User Speedcall - Private | The key is a Speed Call key programmed by the user. The user has designated the number as private, so the Line Type field displays "User Speedcall - Private".
Voice Dial | This key is a Voice Dial (Mitel Speech Server) key