# Attendant Messaging

## Description

Attendant Messaging lets you activate a message waiting condition on a station (see Messaging Dialed and Messaging Callback) from the attendant console. The condition can be queried or canceled by the attendant or by a station user with the appropriate Class of Service.

## Conditions and Feature Interactions

- You cannot invoke message waiting when both the SOURCE (SRC) and DESTINATION (DST) areas share active parties.

- Attendant Messaging does not apply to Conferences.

- Attendant Messaging is not available on the MiVoice Business Console.

## Programming

This feature does not require programming.

## Device Support

All consoles

## Operation

#### 5540 IP Console

To check for message waiting when you are not involved in a call to that station (if you are calling the station no operation is required):

1. Press Function.

2. Press Stn Function.

3. Enter the Number of the station.

4. Press Exit.

To turn message waiting on or off while you are calling a station:

1. Press Msg Waiting.

2. Press Release or Cancel.

To turn message waiting on or off when you are not calling a station:

1. Press Function.

2. Press Stn Function.

3. Enter the number of the station.

4. Press Enter.

5. Press Msg Waiting.

6. Press Exit.