# BWM STATISTICS RESET

## Qualifiers:

None

## Purpose:

Deletes all 15-minute and hourly intervals for Bandwidth Management that are in persistent storage on the MiVoice Business system. It also resets the cumulative counters to zero.

## Details:

If Bandwidth Reporting and Statistics is enabled on the Bandwidth Management form, the historical data resumes when the next 15-minute interval expires.

NOTE: Use this command when the time/date of the switch has been changed.

## Examples:

### Entry: BWM STATISTICS RESET

System Response:

BWM STATS are reset