# HST POLL_HANDOFF

## Qualifiers:

None

## Purpose:

Use this command to periodically display the status of the HST COURTESY_HANDOFF command.

## Details:

Use the HST POLL_HANDOFF command on the controller on which you initiated the Courtesy Handoff.

## Example:

### Entry: HST POLL_HANDOFF

### System Response:

HANDOFF IP GS_COMPLETE

Related Topic

- HST Courtesy_Handoff

- HST CANCEL_HANDOFF