# Group Page (Networked)

## Description

Group Paging can be completed across a network or cluster. This allows a set on system A to page a specific group defined on system B. DISA trunks may initiate a group page.

## Conditions and Feature Interactions

- The group must have all of its members on the same system.

- Meet-Me Answer is not supported across DISA or E&M trunks.

- Networked Group page is not applicable to Symbol Wireless phones.

- Also refer to the Group Page conditions.

## Programming

- If systems are networked, ARS programming must allow sets on one system to dial Page Groups on other systems.

- If systems are clustered, sets initiating a Group Page must be programmed so the directory numbers of the sets in the remote group appear as Remote DNs.

## Device Support

Refer to Group Page.

## Operation

Refer to Group Page.

Related Topics

- Mass Audio Notification