# Phone Model M2616/A2008

When you connect a Nortel Meridian M2616 or A2008 phone to a 3300 CITELlink Gateway and program it as a CITELlink Type2 device, the phone supports the following keys:

Button Label | Function
1 | Cancel
2 | Hold
3 | Prime Line
4 | Feature Key 2
5 | Feature Key 3
6 | Feature Key 4
7 | Feature Key 5
8 | Feature Key 6
9 | Feature Key 7
10 | Program (A2008D, M2216D) Unused (A2008, M2216)
11 | Menu Right (A2008D, M2216D) Unused (A2008, M2216)
12 | Menu Middle (A2008D, M2216D) Unused (A2008, M2216)
13 | Menu Left (A2008D, M2216D) Unused (A2008, M2216)
14 | Down Arrow
15 | Transfer/Conference
16 | Superkey
17 | Message
18 | Handsfree/Mute
19 | Message Indicator Light

Available models:

- A2008/M2616: base models

- A2008D/M2616D: with display