# LGMR SHOW MEMBER

## Qualifiers:

<MemberDN>

## Purpose:

Displays the Last Group Member Routing (LGMR) feature data(CgPN or ANI of the caller, ring group to which the call was made, and the ring group member's number that answered the call) for the ring group member.

## Details:

Applies to ring groups that has the Last Group Member Routing (LGMR) feature enabled.

## Example(s):

### Entry: LGMR SHOW MEMBER 2504

### System Response for an invalid entry or no matching data:

Last Group Member Routing response started:

One or more parameters are incorrect, or no LGMR entries match the parameters.

Last Group Member Routing response completed.

### Entry: LGMR SHOW MEMBER 1873001

### System Response for a valid entry and when matching data is found:

Group: 1876200 CgPN: 1421001 Member: 1873001 Age: 0 minutes.

Group: 1876200 CgPN: 1421002 Member: 1403001 Age: 1 minutes.

Group: 1876200 CgPN: 6135922122 Member: 1403001 Age: 0 minutes.

Last Group Member Routing response completed.