# Set Limits for NuPoint Fax

To set up limits to govern the fax feature:

1. From the Main Menu, select (S) System Maintenance, (R) Reconfiguration, and then (L) Limits COS.

2. Select (C) Choose Limits COS to Modify and enter the number of the LCOS you want to modify.

3. Select (N) Name Selected LCOS and enter a descriptive name (1-15 characters) OR press Enter to accept the displayed name.

To set CNG Tone Detection Length for Walkaway Fax

4. Select (P) Set NuPoint Fax Limits for Selected LCOS.

5. Select (C) Pre-greet Silence Interval to Improve Walkaway CNG Detection =. This parameter should be 0 unless extremely noisy lines affect the CNG detection ability. Enter '.' to set the value to zero.

To set Fax Delivery Limits

6. Still in the NuPoint Fax Limits menu, select (A) Maximum Number of Digits for Telephone Number and enter the maximum number of digits (1-25) allowed in the fax phone number for fax delivery. Include access digits and area code requirements.

7. Select (D) Fax Delivery Retry Frequency and enter the number of retry attempts (0-255) the server will make to deliver a fax.

8. Select (E) Fax Delivery Retry Interval and enter the number of minutes between fax delivery retries.

To set Fax Storage Limits

9. Still in the NuPoint Fax Limits menu, select (B) NuPoint Fax Message Count and enter the maximum number of faxes (1-72) allowed or enter 0 to allow an unlimited number of faxes to be stored.

10. Exit to the Limits Class of Service menu and select (D) Set Mailbox & Message Age Limits for selected LCOS.

11. Select (A) Played Fax Message Retention and enter the number of hours (0-8760) a played fax message is kept if not deleted by the user.

12. Select (B) Unplayed Fax Message Retention and enter the number of hours (0-8760) an unplayed fax message is kept.

13. Select (C) Urgent Fax Message Retention and enter the number of hours (0-8760) an urgent fax message is kept.

14. Select (D) Fax Receipt Retention and enter the number of hours (0-8760) a fax receipt is kept if not deleted by the user.

15. Exit to System Configuration menu to save your changes.