# View LCOS Information

You can view LCOS information through the System Configuration Menu or the Reports Menu.

To display all defined LCOS and the limits parameters that comprise them:

### Using the System Configuration Menu

1. From the Main Menu, select (S) System Maintenance, (R) Reconfiguration, and then (L) Limits COS.

2. To view limits parameters in defined LCOS, select an option (for example, (T) Show More LCOS States), and then enter the number of the LCOS(s) you want to view (1-640) in one of the formats shown here:

3. A single LCOS number, for example 3

4. A range of FCOS numbers, for example 2-4

5. A series of FCOS numbers, for example, 2,4,5,12

6. A for a summary of all FCOS

7. E for a summary of even-numbered FCOS

8. O for a summary of odd-numbered FCOS

9. L for a summary of the lower half of FCOS

10. U for a summary of the upper half of FCOS

3. The server displays a list of all defined LCOS that shows the values set for general limits parameters contained in them.

LCOS to show (? for help)= 1 Max Netq Max User Callr Name Greet Max Msg Net MsgDl 1View # Name Msgs Msgs Bill Len Len Len Len Log Sib Sib Delay Tmout ------------------------------------------------------------------------- 1 Default 200 99 0 5.0 5.0 2 2.0 0 199 199 5 59

4. To view any other limits parameters, select from the following list and enter the LCOS number you want to view:

5. (U) Show Call Placement LCOS States

6. (W) Show NuPoint Fax LCOS states

7. (Y) Show Message Age Limits for Selected LCOS

8. (Z) Show Language for Selected LCOS

### Using the Reports Menu

1. From the Main Menu, select (R) Reports Menu.

2. Select (E) LCOS.

3. At the output routing prompt, select one of the following:

4. C to send the report to the console without pausing

5. P to send the report to the console, pausing as the screen fills,

6. F to send the report to a file on the server,

7. A to append the report to an existing file on the server, or

8. X to exit report output options (no report).

LIMITS CLASS OF SERVICE Wed Oct 28 13:47:08 20XX Max Netq Max User Callr Name Greet Max Msg Net MsgDl 1View # Name Msgs Msgs Bill Len Len Len Len Log Sib Sib Delay Tmout ------------------------------------------------------------ 1 Default 200 99 0 5.0 5.0 2 2.0 0 199 199 5 59 2 NYNEX-Basic 200 99 0 2.0 2.0 2 2.0 0 199 199 5 59 3 NYNEX-Advanced 200 99 0 2.0 2.0 2 2.0 0 199 199 5 59 4 <No name> 200 99 0 5.0 5.0 2 2.0 0 199 199 5 59