# Category 6: Prompts Feature Bits

Prompts feature bits allow the user to interrupt (soft play) prompts and to modify the prompts that the user hears. Also, these feature bits affect some NP Receptionist prompts.

Bit | Description | Required | Incompatible
051 | Do not switch language for outside callers |  |
082 | Soft play (interrupt) message count |  |
083 | Soft play (interrupt) most prompts |  |
097 | *Do not say “I will ring (recipients name)” in NP Receptionist |  |
098 | Say “Press 0” to caller before beep |  |
131 | Don't say limits of liability statement |  |
133 | Don’t say “You may start your msg. now” | 004, 041 |
136 | Don’t say “End of message” | 050 |
138 | Don’t say “Message complete” | 020 |
140 | Say full date when playing messages | 050 | 048, 049, 204
146 | Don’t say “NuPoint Voice storage is full” |  |
157 | Repeat message for answering machine |  |
159 | Say “Press 0 to return to Receptionist” |  |
163 | *Don’t play message count |  |
176 | *Say “Press pound [#] for more options” to callers | 004, 005 |
202 | Do not play mailbox name or extension number | 020 |
208 | *Play reorder tone after CTP or greet-only | 171 or 172 or 062 |
209 | Tone only pager mailbox interface |  |
210 | Numeric display pager mailbox interface |  |
211 | Voice pager mailbox interface |  |
283 | Say number of unplayed messages on last logout |  |
299 | Allow choice of unplayed or saved messages during playback |  |
301 | Enable "Press # when you are finished recording" prompt to make, forward, or answer a message for a mailbox |  |